


1. Open the XLoader app in xLoader-master folder and click button shown.




1. Put the wokwiuno folder on desktop and open the related hex file.




1. Device choose Uno(ATmega328) and Baud rate is 115200.




1. Choose the com port where the Arduino uno is connected.



1. After confirm the com port is correct, click Upload.



1. You can check your connected Arduino uno com port with Device Manager.
2. In case the PC and UNO not connected, try install driver CH341SER.